Dear Vendor,
Kindly send your best priced offer for the below outdoor power cables with the following specifications and quantities no later than Tuesday 7 June 2026 before 12:00 PM:
Technical Specifications:
1. Conductors: Copper, circular stranded, conforming to the applicable requirements of IEC 60228.
1. Insulation: XLPE thermosetting material, conforming to the applicable requirements of IEC 60502-1.
1. Temperature Rating: PVC insulation and thickness to comply with IEC 60502, suitable for continuous operation at 90°C.
1. Assembly: Two insulated cores laid up together with non-hygroscopic fillers compatible with the insulation material, covered with an extruded PVC bedding layer.
1. Armor: Galvanized steel or aluminum wire armor applied helically over the bedding, in accordance with IEC 60502.
1. Outer Sheath: Extruded PVC, Type ST2, conforming to IEC 60502-1.
Required Quantity:
1. 2 × 10 AWG Outdoor Power Cable: 10,000 meters
Commercial Requirements:
1. Delivery: Within 20 calendar days from the date of Purchase Order issuance. This is a mandatory requirement and will be considered a critical evaluation criterion. MIC2 reserves the right to reject any delivery made later than 30 calendar days after the PO issuance.
1. Offer Submission Deadline: One week from the RFQ issuance date.
Delivery time of all above works shall be mentioned in the offer.

Offers should be submitted in USD currency to be paid by bank transfer in LBP at time of payment as per current rate.

Data sheets must be submitted along with your offer.

The sealed envelope should be submitted by hand and marked visibly with the reference TechProcurement /OUTDOORCABLES /1/7/2026 and submitted 
to the following address:
 
Procurement Department 8th floor
Beirut Central Building (Touch Building)
Plot # 1526 / Bashoura - Block B
Fouad Chehab Avenue
Beirut
PO. BOX 175051

For contact: Rabih  03 620 922

Best Regards,

