RAM configuration for the Cisco server RFQ

	Product Name
	Product Quantity

	Cisco Memory (RAM): 128 GB LRDIMM (UCS-ML-128G4RT-H)
	8

	Fiber Channel HBA: 1 x 16 Gb Dual-Port HBA (Emulex: UCSC-PCIE-BD16GF)
	1



Killing Factors: 

	Killing Factors
	Fully Comply
	Reference

	The Bidder must be a Cisco preferred partner or above. Certifications should be provided.
	 
	 

	Installation and configuration should be performed directly with the existing partner handling the support on the current Cisco infrastructure.
	 
	 

	Cisco Certifications for Minimum 3 Engineers. 
	 
	 

	MAF Letter from Cisco should be provided including the name of the partner and the RFQ.
	
	



