Dear Vendor,

Kindly send your best priced quotation for the supply of waveguides from different frequencies, IF cables, and their related accessories to support the maintenance and implementation of microwave transmission links.
These materials will be used for corrective and preventive maintenance activities on live microwave sites to ensure continued link availability and performance.
	Item description
	Quantity

	Microwave Accessory,Flexible Waveguide,18/23/26G,0.9m,PBR220,With English doc
	24

	Microwave Accessory,Flexible Waveguide,28/32/38G,0.9m,PBR320,With English doc
	24

	Microwave Accessory,Flexible Waveguide,15G,0.9m,PBR140,With English doc
	24

	Microwave Accessory,Flexible Waveguide,10/11G,1.8m,PBR100,With English doc
	8

	Microwave Accessory,Flexible Waveguide,10/11G,0.9m,PBR100,With English doc
	8

	Twistflex Hanger

	200

	Coaxial Cable, Copper-clad Aluminium Wire,50ohm,7.6mm,4.8mm,1.8mm, Black, 5D

	20,000 meter

	Patch Cord Accessories of Double IF (5D)

	200



Below are the technical specs for the waveguides required:

	Parameter
	Specification

	Type
	Flexible rectangular microwave waveguide

	Application
	Microwave transmission maintenance

	Length
	0.9 meters

	Frequency Range
	As specified for each requested frequency band

	Waveguide Size
	Standard WR series corresponding to the operating frequency

	Material
	High-conductivity brass or copper with corrosion-resistant finish

	Flanges
	Standard IEC/CPR/UBR or equivalent, factory assembled

	VSWR
	≤ 1.15:1

	Insertion Loss
	Low-loss design as per manufacturer's specifications

	Operating Temperature
	-40°C to +70°C

	Environmental Protection
	Suitable for indoor and outdoor installations



All waveguides should be compatible with Andrew and HATA antennas.
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Suppliers should provide a sample for technical acceptance.
The sealed envelope should be submitted by hand no later than Monday 3 August 2026 before 12:00 PM and marked visibly with the reference TechProcurement /WAVEGUIDESIF /24/7/2026 and submitted 
to the following address:
Procurement Department 8th floor
Beirut Central Building (Touch Building)
Plot # 1526 / Bashoura - Block B
Fouad Chehab Avenue
Beirut
PO. BOX 175051

For contact:  Mohamed  70 703 181

Best Regards,
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